SYS
SYS0000I: Y N A R I
SYS0396E: The system cannot find the COUNTRY.SYS file.
SYS3100I: This version of the CD-ROM file system (CDFS) will not run
on OS/2 Warp version 4.
SYS3101I: The CD-ROM file system (CDFS) driver with debug statistics
(%1) is loading.
SYS3102I: The CD-ROM file system (CDFS) driver with debug (%1)
is being loaded.
SYS3103I: The CD-ROM file system (CDFS) driver with statistics (%1)
is being loaded.
SYS3104I: The CD-ROM file system (CDFS) driver (%1) for OS/2 Warp version 4
is being loaded.
SYS3105I: The CD-ROM file system (CDFS) received an unrecognized
error code from the device driver.  Refer to the documentation that
came with your device driver.
SYS3106I: A parameter in the CD-ROM file system (CDFS) is invalid.
SYS3107I: The minimum number of cache-buffer sectors (1) is being used.
You specified fewer sectors than the minimum number allowed by the
CD-ROM file system (CDFS).  Your program will continue to run with the
default minimum number.  The minimum number of sectors is 1.
SYS3108I: The communication port being used for debug is %1.
SYS3109I: The maximum number of cache-buffer sectors is being used.
You specified more sectors than are allowed by the CD-ROM file system
(CDFS).  Your program will continue to run with the default maximum
number of sectors that can be used at the same time, which is 32.
SYS3110I: You specified fewer file sectors to read than are
allowed.  Your program will continue to run with the default minimum
number, which is 1 sector.
SYS3111I: You specified more file sectors to read than are
allowed.  Your program will continue to run with the default maximum
number of sectors that can be read at once, which is 32.
SYS3112I: The CD-ROM file system (CDFS) is using the primary volume
descriptor.
SYS3113I: The CD-ROM file system (CDFS) is using the secondary volume
descriptor that you specified.
SYS3114I: The CD-ROM file system (CDFS) is using %1 of the 64KB
cache buffers.
SYS3115I: The CD-ROM file system (CDFS) is reading %1 sectors with
each read.
SYS3116I: The CD-ROM file system (CDFS) could not be loaded.
SYS3117I: The CD-ROM file system (CDFS) has had a total memory
allocation failure.  This file system driver (FSD) operation failed.
SYS3118I: The CD-ROM file system (CDFS) has had a partial memory
allocation failure.  %1 of %2 cache segments were used.
SYS3119I: The CD-ROM file system (CDFS) is unable to read global
InfoSeg.
